567—122.10 (455B,455D) Design requirements for CRT recycling facilities. A CRT recycling facility shall be designed and constructed to meet the following requirements:
	 122.10(1) CRT recycling facilities shall be enclosed by walls, a roof, and a floor satisfactory to:
	  a.   	 Prevent litter from exiting the building.
	  b.   	 Keep precipitation out of the building.
	 122.10(2) A CRT recycling facility shall maintain a separation between stormwater and liquids generated inside the building.
	 122.10(3) Discarded CRTs shall be demanufactured and processed in an area where hazardous materials can be contained.
	 122.10(4) A sign shall be posted at the primary entrance to the facility. The sign shall be a minimum of 8½ × 11 inches and visible from the outside of the building at approximately eye level. The lettering shall be a minimum of 1-inch high and state the following information:
	  a.   	 Name and permit number of facility.
	  b.   	 Telephone number of emergency contact person(s).
	 122.10(5) A CRT recycling facility may store discarded CRTs and materials derived from discarded CRTs outdoors if the following conditions are met:
	  a.   	 The facility has a stormwater permit, if applicable.
	  b.   	 The material is not harboring or attracting vectors.
	  c.   	 Litter is contained within the storage area or unit.
	  d.   	 The discarded CRTs and materials derived from discarded CRTs are not broken CRTs or CRT glass.
[ARC 8679B, IAB 4/7/10, effective 7/1/10]