567—118.7 (455B,455D) Fixed facilities and mobile operations. The following removal and disposal requirements must be met by both fixed facilities and mobile operations.
	 118.7(1) Demanufacturing of appliances must take place on an impervious floor (including but not limited to concrete, ceramic tile, or metal, but not wood). Any spills must be contained and picked up with proper equipment and procedures and be disposed of properly.
	 118.7(2) The point of demanufacturing must be located at least 50 feet from a well and any water of the state.
	 118.7(3) The facility must be located above the 100-year floodwater elevation.
	 118.7(4) A permanent facility must meet local zoning requirements.
	 118.7(5) An applicant must establish a unique marking system, to be submitted with the permit application for department approval, signifying that all refrigerants, PCB-containing articles, and mercury-containing components have been removed. The unique marking system must be a minimum of nine inches by nine inches and must be applied to the appliances after demanufacturing.