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ARC 0595D
INSPECTIONS AND APPEALS DEPARTMENT[481]
Adopted and Filed
Rulemaking related to dust-lead hazards and training
    The Department of Inspections, Appeals, and Licensing hereby amends Chapter 470, “Lead-Based Paint Activities,” Iowa Administrative Code.
Legal Authority for Rulemaking
    This rulemaking is adopted under the authority provided in Iowa Code chapter 10A.
State or Federal Law Implemented
    This rulemaking implements, in whole or in part, Iowa Code chapter 10A.
Purpose and Summary
    This rulemaking amends Chapter 470 to implement the United States Environmental Protection Agency’s (EPA’s) rule regarding the definition of “dust-lead hazard.”
    This rulemaking amends the rules to provide a clearer guideline for lead professionals regarding training and certification to perform lead-based paint activities and references to federal law.
Public Comment and Changes to Rulemaking
    Notice of Intended Action for this rulemaking was published in the Iowa Administrative Bulletin on July 22, 2026, as ARC 0447D. No public comments were received. No changes from the Notice have been made.
Adoption of Rulemaking
    This rulemaking was adopted by the Department on August 26, 2026.
Fiscal Impact
     This rulemaking has no fiscal impact to the State of Iowa. 
Jobs Impact
    After analysis and review of this rulemaking, no impact on jobs has been found.
Waivers
    Any person who believes that the application of the discretionary provisions of this rulemaking would result in hardship or injustice to that person may petition the Department for a waiver of the discretionary provisions, if any, pursuant to 7—Chapter 2504.
Review by Administrative Rules Review Committee
    The Administrative Rules Review Committee, a bipartisan legislative committee which oversees rulemaking by executive branch agencies, may, on its own motion or on written request by any individual or group, review this rulemaking at its regular monthly meeting or at a special meeting. The Committee’s meetings are open to the public, and interested persons may be heard as provided in Iowa Code section 17A.8(6).
Effective Date
    This rulemaking will become effective on October 21, 2026.
    The following rulemaking action is adopted:
    ITEM 1.  Amend rule 481—470.2(10A), definitions of “Clearance level,” and “Dust-lead hazard,” as follows:
    “Clearance level” means the value at which the amount of lead in dust on a surface following completion of interim controls, lead abatement, paint stabilization, standard treatments, ongoing lead-based paint maintenance, rehabilitation, or renovation is a dust-lead hazard and fails clearance testing. The clearance level for a single-surface dust sample from a floor is greater than or equal to 10 5 micrograms per square foot. The clearance level for a single-surface dust sample from an interior windowsill is greater than or equal to 100 40 micrograms per square foot. The clearance level for a single-surface dust sample from a window trough is greater than or equal to 400 100 micrograms per square foot.
    “Dust-lead hazard” means surface dust in residential dwellings or child-occupied facilities that contains a mass-per-area concentration of lead greater than or equal to 10 5 micrograms per square foot on floors, 100 40 micrograms per square foot on interior windowsills, and 400 100 micrograms per square foot on window troughs based on wipe samples. A dust-lead hazard is present in a residential dwelling or child-occupied facility when the weighted arithmetic mean lead loading for all single-surface or composite samples of floors and interior windowsills is greater than or equal to 10 5 micrograms per square foot on floors, 100 40 micrograms per square foot on interior windowsills, and 400 100 micrograms per square foot on window troughs based on wipe samples. A dust-lead hazard is present on floors, interior windowsills, or window troughs in an unsampled residential dwelling in a multifamily dwelling if a dust-lead hazard is present on floors, interior windowsills, or window troughs, respectively, in at least one sampled residential unit on the property. A dust-lead hazard is present on floors, interior windowsills, or window troughs in an unsampled common area in a multifamily dwelling if a dust-lead hazard is present on floors, interior windowsills, or window troughs, respectively, in at least one sampled common area in the same common area group on the property.
    ITEM 2.  Amend subrule 470.4(14) as follows:
    470.4(14) To be approved for A refresher training of course for sampling technicians, lead abatement contractors, lead abatement workers, and project designers, a course must be at least eight hours of training hours. To be approved for Pursuant to the recertification requirements of subrule 470.5(6), a refresher training of course for lead inspector/risk assessors and elevated blood lead (EBL) inspector/risk assessors who completed an approved 24-hour training course, a course must be at least 8 hours of training hours. Pursuant to meet the recertification requirements of subrule 470.5(3). To be approved for 470.5(6), a refresher training of course for lead inspector/risk assessors and elevated blood lead (EBL) inspector/risk assessors to meet the recertification requirements of subrule 470.5(6), a course must be at least 16 hours of training hours. To be approved for A refresher training of course for lead-safe renovators, a course must be at least four hours and must include a hands-on component of training. All refresher training courses shall cover at least the following topics:
    a.  to d. No change.
    ITEM 3.  Amend rule 481—470.12(10A) as follows:
481—470.12(10A) References to federal law. Unless otherwise specified, all references in this chapter to the United States Code or to the Code of Federal Regulations are to those provisions in effect on July 1, 2024 2026.

[Filed 8/26/26, effective 10/21/26]
[Published 9/16/26]
EDITOR’S NOTE: For replacement pages for IAC, see IAC Supplement 9/16/26.
[bookmark: lastARC]
	
	
	, v _


