327G.13  Signals at road crossings.
  A bell and a horn shall be placed on each locomotive engine operated on any railway, which horn shall be sounded at least one thousand feet before a road crossing is reached, and after the sounding of the horn the bell shall be rung continuously until the crossing is passed; but at street crossings within the limits of cities the sounding of the horn may be omitted, unless required by ordinance or resolution of the council thereof; and the company shall be liable for all damages which shall be sustained by any person by reason of such neglect.
[C97, §2072; C24, 27, 31, 35, 39, §8018; C46, 50, 54, 58, 62, 66, 71, 73, 75, §478.19; C77, 79, 81, §327G.13]