321.417  Single-beam road-lighting equipment.
  Headlamps arranged to provide a single distribution of light not supplemented by auxiliary driving lamps shall be permitted on motor vehicles manufactured and sold prior to July 1, 1938, in lieu of multiple-beam road-lighting equipment specified in section 321.409 if the single distribution of light complies with the following requirements and limitations:
  1.  The headlamps shall be so aimed that when the vehicle is not loaded none of the high-intensity portion of the light shall at a distance of twenty-five feet ahead project higher than a level of five inches below the level of the center of the lamp from which it comes, and in no case higher than forty-two inches above the level on which the vehicle stands at a distance of seventy-five feet ahead.
  2.  The intensity of the light shall be sufficient to reveal persons and vehicles at a distance of at least two hundred feet.
[C24, 27, 31, 35, §5049; C39, §5034.26; C46, 50, 54, 58, 62, 66, 71, 73, 75, 77, 79, 81, §321.417]
2010 Acts, ch 1069, §97
Referred to in §321.1, 321.418