364.23  Energy-efficient lighting required.
  All city-owned exterior flood lighting, including but not limited to street and security lighting but not including era or period lighting which has a minimum efficiency rating of fifty-eight lumens per watt and not including stadium or ball park lighting, shall be replaced, when worn-out, exclusively with high pressure sodium lighting or lighting with equivalent or better energy efficiency as approved in rules adopted by the utilities commission. In lieu of the requirements established for replacement lighting under this section, stadium or ball park lighting shall be replaced, when worn-out, with the most energy-efficient lighting available at the time of replacement which may include metal halide, high-pressure sodium, or other light sources which may be developed.
89 Acts, ch 297, §6
; 91 Acts, ch 253, §16
; 92 Acts, ch 1233, §3
; 2023 Acts, ch 19, §2665; 2024 Acts, ch 1170, §369
Referred to in §474.5
Code editor directive applied