CHAPTER 811
HIGHWAY-RAILROAD GRADE CROSSING WARNING DEVICES
[Prior to 6/3/87, Transportation Department [820]—(10,B)Ch 2]
761—811.1(307) Standards. All highway-railroad grade crossing warning devices installed shall conform to Part 8, “Traffic Controls for Railroad and Light Rail Transit Grade Crossings,” of the “Manual on Uniform Traffic Control Devices” as adopted in 761—Chapter 130.
This rule is intended to implement Iowa Code sections 307.26(7)“b,” 321.252 and 327G.2.
[ARC 6710C, IAB 11/30/22, effective 1/4/23]
761—811.2(307) Contact information. Information about this chapter may be obtained by contacting the department at the following address: Modal Transportation Bureau, Iowa Department of Transportation, 800 Lincoln Way, Ames, Iowa 50010; telephone (515)239-1108.
This rule is intended to implement Iowa Code section 307.26.
[ARC 6710C, IAB 11/30/22, effective 1/4/23]
[Filed 8/24/82, Notice 7/7/82—published 9/15/82, effective 10/20/82]
[Filed 10/2/85, Notice 8/14/85—published 10/23/85, effective 11/27/85]
[Filed 5/11/87, Notice 3/11/87—published 6/3/87, effective 7/8/87]
[Filed 4/17/96, Notice 3/13/96—published 5/8/96, effective 6/12/96]
[Filed 7/15/03, Notice 5/14/03—published 8/6/03, effective 9/10/03]
[Filed ARC 6710C (Notice ARC 6575C, IAB 10/5/22), IAB 11/30/22, effective 1/4/23]