CHAPTER 811
HIGHWAY-RAILROAD GRADE CROSSING WARNING DEVICES
[Prior to 6/3/87, Transportation Department [820]—(10,B)Ch 2]
761—811.1(307) Standards. All highway-railroad grade crossing warning devices installed shall conform to Part 8, “Traffic Controls for Highway-Rail Grade Crossings,” of the “Manual on Uniform Traffic Control Devices” as adopted in 761—Chapter 130.
This rule is intended to implement Iowa Code paragraph 307.26(5)“b” and sections 321.252 and 327G.2.
[Filed 8/24/82, Notice 7/7/82—published 9/15/82, effective 10/20/82]
[Filed 10/2/85, Notice 8/14/85—published 10/23/85, effective 11/27/85]
[Filed 5/11/87, Notice 3/11/87—published 6/3/87, effective 7/8/87]
[Filed 4/17/96, Notice 3/13/96—published 5/8/96, effective 6/12/96]
[Filed 7/15/03, Notice 5/14/03—published 8/6/03, effective 9/10/03]