CHAPTER 452
REFLECTIVE DEVICES ON SLOW-MOVING VEHICLES
[Appeared as Ch 3, Department of Public Safety, 1973 IDR]
[Prior to 6/3/87, Transportation Department[820]—(07,E) Ch 3]
761—452.1(321) Slow-moving vehicle. Rescinded IAB 4/5/00, effective 5/10/00.
761—452.2(321) Required equipment. Rescinded IAB 4/5/00, effective 5/10/00.
761—452.3(321) Alternative reflective device. If a person operating a vehicle drawn by a horse or mule objects for religious reasons to using a reflective device that complies with the standards of the American Society of Agricultural Engineers, the vehicle may be identified by an alternative reflective device that is in compliance with the following:
	452.3(1) The alternative reflective device shall consist of one-inch-wide strips applied to the rear of the vehicle. The combined length of the strips shall be at least 72 inches. The strips, when applied, shall approximate the outline of the vehicle.
	452.3(2) The reflective material may be black, gray, silver or white in color, but must reflect white when illuminated by other vehicles’ headlamps.
	452.3(3) The reflective material shall be visible from a distance of not less than 500 feet from the rear of the vehicle when illuminated by other vehicles’ headlamps.
	452.3(4) The reflective material shall be kept free of dirt and debris.
This rule is intended to implement Iowa Code section 321.383(2).
[Editorial change: IAC Supplement 2/24/21]
[Filed 2/22/72; transferred to Department of Transportation 7/1/75]
[Filed 5/11/87, Notice 3/11/87—published 6/3/87, effective 7/8/87]
[Filed 3/9/00, Notice 1/26/00—published 4/5/00, effective 5/10/00]
[Editorial change: IAC Supplement 2/24/21]