CHAPTER 504
STANDARDS FOR ELECTRICAL WORK
661—504.1(103) Installation requirements. The provisions of the National Electrical Code, 2011 edition, published by the National Fire Protection Association, 1 Batterymarch Park, Quincy, MA 02169-7471, are adopted as the requirements for electrical installations performed by persons licensed pursuant to 661—Chapters 500 through 503 and to installations subject to inspection pursuant to Iowa Code chapter 103 with the following amendments:
	504.1(1) Add the following exceptions to section 210.8, paragraph (A), subparagraph (2):
	a. 	Exception No.	1 to (2): Receptacles that are not readily accessible.
	b. 	Exception No.	2 to (2): A single receptacle or a duplex receptacle for two appliances located within dedicated space for each appliance that, in normal use, is not easily moved from one place to another and that is cord-and-plug connected in accordance with 400.7(A)(6), (A)(7), or (A)(8).
	c. 	Receptacles installed under the exceptions to 210.8(A)(2) shall not be considered as meeting the requirements of 210.52(G).
	504.1(2) Add the following exceptions to section 210.8, paragraph (A), subparagraph (5):
	a. 	Exception No.	2 to (5): Receptacles that are not readily accessible.
	b. 	Exception No.	3 to (5): A single receptacle or a duplex receptacle for two appliances located within dedicated space for each appliance that, in normal use, is not easily moved from one place to another and that is cord-and-plug connected in accordance with 400.7(A)(6), (A)(7), or (A)(8).
	c. 	Receptacles installed under the exceptions to 210.8(A)(5) shall not be considered as meeting the requirements of 210.52(G).
This rule is intended to implement Iowa Code chapter 103.
[ARC 9825B, IAB 11/2/11, effective 1/1/12]
[Filed emergency 12/17/07—published 1/16/08, effective 1/1/08]
[Filed 10/29/08, Notice 9/24/08—published 11/19/08, effective 1/1/09]
[Filed ARC 9825B (Notice ARC 9630B, IAB 7/27/11), IAB 11/2/11, effective 1/1/12]