199—21.14(476) Meter testing for sanitary sewage disposal service.  If a utility uses separate meters to measure the volume of sewage disposal, the separate meters shall be tested in substantial conformity with the requirements of rule 199—21.6(476).
[ARC 4873C, IAB 1/15/20, effective 2/19/20]