21—85.11(215) Scale pit. 
    85.11(1) In the construction of a scale pit, walls must be of reinforced concrete. A slab floor must be installed in the pit. The floor must be at least 12 inches thick with a minimum of grade 40 reinforcement rod running into all piers and sidewalls, installed according to the manufacturer’s specifications. There shall be an approach at each end of the scale of not less than ten feet, and said approach shall be of reinforced concrete 12 inches thick on a level with the scale deck. A slope of a one-inch drop across the ten-foot span may be allowed for drainage.
    85.11(2) Electronic scales shall have a vertical clearance of not less than four feet from the floor line to the bottom of the I-beam of the scale bridge, thus providing adequate access for inspection and maintenance. The load-bearing supports of all scales installed in a fixed location shall be constructed to ensure the strength, rigidity and permanence required for proper scale performance.
This rule is intended to implement Iowa Code section 215.15.
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