21—85.50(214,214A,215) Blender pumps. Motor fuel blender pumps or blender pumps installed or modified after November 1, 2008, which sell both ethanol blended gasoline classified as higher than E-15 and gasoline need to have at least two hoses per pump to separate registered gasoline fuels from flex fuels.
This rule is intended to implement Iowa Code section 214A.2.
[ARC 7628B, IAB 3/11/09, effective 4/15/09; ARC 0079C, IAB 4/4/12, effective 3/16/12; ARC 6216C, IAB 2/23/22, effective 5/1/22]