875—72.4 (89A) Electric elevators. The provisions contained in ASME A17.1, part 2, are adopted by reference.