875—72.5 (89A) Hydraulic elevators. The provisions contained in ASME A17.1, part 3, are adopted by reference.