875—72.6 (89A) Power sidewalk elevators. The provisions contained in ASME A17.1, section 5.5, are adopted by reference.