567—101.306(455B) Operating requirements. Unless otherwise specified within a permit, a CCR landfill shall be operated in accordance with the provisions of 567—100.9(455B,455D). No wastes shall be deposited within 300 feet of an inhabitable residence or a commercial enterprise unless there is a written agreement with the property owner(s) allowing a lesser distance that has been filed with the local county recorder under the adjoining property or within 50 feet of the property boundary under any circumstances. An operations plan shall be prepared and submitted to the department that includes the following.
    101.306(1) An identification of the area(s) to be filled during the period for which a permit is being requested.
    101.306(2) The method(s) that will be utilized to prevent illicit municipal or putrescible solid wastes from being deposited as a result of mixing with authorized waste brought to the site.
    101.306(3) The frequency, extent, and method of spreading and compacting the waste; the optimum layer thickness; and the size and slope of the operating face.
    101.306(4) A description of the operating procedures from the arrival of waste to the site through unloading, placing, and closure to control fugitive dust, erosion, and contact water. If the methods used do not adequately control dust, contact water, and erosion, the department may require site-specific controls including a soil cover.
    101.306(5) Detailed procedures for the removal of waste from the CCR landfill for beneficial reuse, if applicable.
    101.306(6) Operating procedures for stormwater, contact water, and leachate management systems.
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