567—102.605(455D) Operations. The following removal and disposal requirements must be met by both fixed facilities and mobile operations.
    102.605(1) Demanufacturing of appliances must take place on an impervious floor, including but not limited to concrete, ceramic tile, or metal, but not including wood. Any spills must be contained and picked up with proper equipment and procedures and be disposed of properly.
    102.605(2) The point of demanufacturing must be located at least 50 feet from a well and any water of the state.
    102.605(3) The facility must be located above the 100-year floodwater elevation.
    102.605(4) A permanent facility must meet local zoning requirements.
    102.605(5) Every operation must have a unique mark that signifies all refrigerants, PCB-containing articles, and mercury-containing components have been removed. The unique mark must be a minimum of nine inches by nine inches. The unique mark must be applied to appliances after demanufacturing.
[ARC 0483D, IAB 8/19/26, effective 9/23/26]
	
	
	, v _


