567—102.612(455D) Appliance demanufacturing facility closure requirements. In addition to the requirements in 567—100.10(455B), an appliance demanufacturing facility shall do the following prior to closure:
    1.   Remove all appliances that have not been demanufactured.
    2.   Properly dispose of all refrigerant, PCBs, mercury, and all hazardous materials.
    3.   Submit an annual report covering January 1, through the last disposal of hazardous materials, PCBs, and refrigerant.
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