491—12.9 (99F) Slot machine container and key. Each slot machine shall have a container(s) that is housed in a locked compartment(s) separate from any other compartment of the slot machine.
	 12.9(1) Each container shall:
	  a.   	 Have a lock securing the contents of the container, the key to which shall be logged out by the count team or employees authorized by the internal controls to address container malfunction issues.
	  b.   	 Have a lock to each compartment securing the container to the slot machine, the key to which shall be different from the key in paragraph 12.9(1)“a” and shall be logged out by the drop team, employees authorized by the internal controls to address container malfunction issues, or employees transporting container(s) according to rule 491—12.13(99F).
	  c.   	 Be identified at the time of removal by a number corresponding to the number of the slot machine from which the container is removed.
	 12.9(2) Keys referred to in subrule 12.9(1) shall be maintained and controlled by the security department in a secured area. The facility shall establish a log-out procedure for all keys removed from the secured area.
	 12.9(3) Other keys to each slot machine or any device connected thereto which may affect the operation of the slot machine shall be maintained in a secure place and controlled by the slot department.
[ARC 8029B, IAB 8/12/09, effective 9/16/09; ARC 9018B, IAB 8/25/10, effective 9/29/10]