571—38.25 (462A) Number designating passenger capacity. The passenger capacity of boats as assigned by the commission shall be painted or attached to the starboard side (the right side while in boat and facing the bow) of boat within nine inches of transom in three-inch or larger block numbers in a color contrasting to the boat color so that the numbers ride above the water line when boat is fully loaded.