661—301.4 (103A) Mechanical requirements. The provisions of the International Mechanical Code, 2006 edition, published by the International Code Council, 5203 Leesburg Pike, Suite 600, Falls Church, VA 22041, are hereby adopted by reference as the requirements for the design, installation, maintenance, alteration, and inspection of mechanical systems that are permanently installed and utilized to provide control of environmental conditions and related processes within buildings, with the following amendments:
Delete chapter 1.
Delete section 403 and insert in lieu thereof the following new section:
SECTION 403
MECHANICAL VENTILATION
Mechanical ventilation systems shall be designed in accordance with the provisions of ASHRAE Standard 62.1-2004, “Ventilation for Acceptable Indoor Air Quality,” published by the American Society of Heating, Refrigerating and Air-Conditioning Engineers, 1791 Tullie Circle, N.E., Atlanta, GA 30329.
Delete appendices A and B.
Delete all references to the “International Plumbing Code” and insert in lieu thereof “state plumbing code.”
Delete all references to the “ICC Electrical Code” and insert in lieu thereof “National Electrical Code, 2005 edition.”