661—5.652 (100) Exits and occupancy load. Rescinded IAB 11/22/06, effective 1/1/07.