761—811.1(307) Standards. All highway-railroad grade crossing warning devices installed shall conform to Part 8, “Traffic Controls for Railroad and Light Rail Transit Grade Crossings,” of the “Manual on Uniform Traffic Control Devices” as adopted in 761—Chapter 130.
This rule is intended to implement Iowa Code sections 307.26(7)“b,” 321.252 and 327G.2.
[ARC 6710C, IAB 11/30/22, effective 1/4/23]