21—85.26(215) Delivery outlets. No means shall be provided by which any measured liquid can be diverted from the measuring chamber of the meter or the discharge line therefrom. However, two or more delivery outlets may be installed, if automatic means is provided to ensure that liquid can flow from only one such outlet at one time and the direction of flow for which the mechanism may be set at any time is definitely and conspicuously indicated.
This rule is intended to implement Iowa Code section 215.18.
[ARC 7129C, IAB 12/13/23, effective 1/17/24]