875—93.3 (89) Maximum working pressure. The maximum allowed working pressure is to be determined by rule 875—92.4(89).