21—69.9 (192) Safety regulations. The usual safety regulations for a 220-volt weatherproof electrical connection for a milk pump shall be followed. The switch box shall be placed on the inside wall of the milk room.