567—72.7 (455B) Sanitary landfills. The following criteria shall apply to sanitary landfills.
	 72.7(1) Location. Sanitary landfills shall not be located so as to individually or collectively conflict with 567—75.4(455B) governing the establishment of encroachment limits.
	 72.7(2) Flood protection. Flood protection for the active working portion of the sanitary landfill shall be provided to the level necessary for high damage potential buildings or building complexes.