875—91.19(89) ASME stamp.  All objects shall bear the appropriate ASME stamp. Objects shall not be utilized in a manner inconsistent with the stamp.
[ARC 8283B, IAB 11/18/09, effective 1/1/10; ARC 3903C, IAB 7/18/18, effective 9/1/18]