567—118.8 (455B,455D) Training. Beginning January 1, 2003, at least one owner or employee of an appliance demanufacturing facility must have a training certificate from a department-approved training course. A person who has completed the department-approved training course must be on site at all times when discarded appliances are being demanufactured. The training will, at a minimum, cover the following topics.
	  1. 	 State and federal regulations for the removal, storage, transportation, and disposal of refrigerant, PCB-containing articles, mercury-containing components, and asbestos from appliances.
	  2. 	 Record-keeping requirements.
	  3. 	 Safety precautions for handling appliances and hazardous materials.
	  4. 	 Spill prevention and cleanup procedures appropriate for appliance demanufacturing.
	  5. 	 The proper methods of loading and unloading discarded appliances.
	  6. 	 General demanufacturing procedures.