215.15  Scale pit.
  Scale pit shall have proper room for inspector or service person to repair or inspect scale. Scale pit shall remain dry at all times and adequate drainage shall be provided for the purpose of inspecting and cleaning.
[C50, 54, 58, 62, 66, 71, 73, 75, 77, 79, 81, §215.15]