216C.9  Curb ramps and sloped areas for persons with disabilities.
  1.  If a street, road, or highway in this state is newly built or reconstructed, a curb ramp or sloped area shall be constructed or installed at each intersection of the street, road, or highway with a sidewalk or path. If a sidewalk or path in this state is newly built or reconstructed, a curb ramp or sloped area shall be constructed or installed at each intersection of the sidewalk or path with a street, highway, or road.
  2.   Curb ramps and sloped areas that are required pursuant to this section shall be constructed or installed in compliance with applicable federal requirements adopted in accordance with the federal Americans With Disabilities Act, including but not limited to the guidelines issued by the federal architectural and transportation barriers compliance board.
[C75, 77, 79, 81, §601D.9]

93 Acts, ch 95, §7; 96 Acts, ch 1129, §37; 2010 Acts, ch 1079, §7; 2010 Acts, ch 1193, §43