321E.9B  Special alternative energy multi-trip permit.
  Subject to the discretion and judgment provided for in section 321E.2, a multi-trip permit shall be issued for operation of vehicles in accordance with the following provisions:
  1.  Vehicles with an indivisible load having an overall length not to exceed two hundred twenty-five feet, an overall width not to exceed sixteen feet, a height not to exceed sixteen feet, and a total gross weight not to exceed two hundred fifty-six thousand pounds may be moved on highways specified by the permit-issuing authority to an alternative energy construction site or staging area for alternative energy transportation, provided the gross weight on any one axle shall not exceed twenty thousand pounds.
  2.  The special alternative energy multi-trip permit shall not exceed twelve months in duration.
  3.  The permit-issuing authority shall have discretion to include restrictions and require special considerations, such as responsibility for protection or repair of the roadway and bridges, prior to issuance of the permit.
2008 Acts, ch 1124, §14, 40; 2013 Acts, ch 49, §8