327F.34  Windshields on power track cars.
  All railroads shall be required to equip any regularly assigned section track power car used on its tracks with a transparent windshield sufficient in width and height to reasonably protect said employees; which windshield shall be of safety glass and shall be equipped with manually controlled windshield wiper which will remove rain, snow and sleet from the windshield while such power track car is in motion and tops of such material and construction to adequately provide reasonable protection for said employees from the inclement weather.
[C66, 71, 73, 75, §477.61; C77, 79, 81, §327F.34]