478.25  Wire crossing railroads — supervision.
  The utilities board shall have general supervision over any and all wires whatsoever crossing under or over any railway track and shall make rules prescribing the manner in which such wires shall cross such track; but in no case shall the board prescribe a less height for any wire than twenty-two feet above the top of the rails of any railroad track.
[S13, §2120-d, -e, -h; C24, 27, 31, 35, 39, §8333; C46, 50, 54, 58, 62, §489.24; C66, 71, 73, 75, §489.25; C77, 79, 81, §478.25]