761—511.8 (321,321E) Annual oversize/overweight permits. Annual oversize/overweight permits are issued for indivisible vehicles or indivisible loads for travel when either the dimensions or the weight or both the dimensions and the weight exceed statutory limits. Travel is not allowed on the interstate. However, a carrier moving under this annual oversize/overweight permit may operate under the same restrictions as an annual permit under rule 511.7(321,321E) when the vehicle meets the dimensions required by that rule. Routing is subject to embargoed bridges and roads and posted speed limits. Annual oversize/overweight permits are issued for the following:
	 511.8(1) Vehicles with indivisible loads, including construction machinery, mobile homes and factory-built structures, provided the following are not exceeded:
	  a.   	 Width. 13 feet 5 inches.
	  b.   	 Length. 120 feet 0 inches.
	  c.   	 Height. 15 feet 5 inches.
	  d.   	 Weight. See rule 511.12(321,321E).
	  e.   	 Routing. The owner or operator shall select a route using a vertical clearance map, kip map, bridge embargo map and detour and road embargo map provided by the department. Detour and road embargo information may also be found on the Internet at www.511ia.com. The owner or operator shall contact the department by telephone at 1-800-925-6469 between 8 a.m.	and 4 p.m., Monday through Thursday, except for legal holidays or at any other time at (515)237-3206 prior to making the move to verify that the owner or operator is using the most recent information.
	 511.8(2) Reserved.
This rule is intended to implement Iowa Code sections 321.454, 321.456, 321.457, 321.463, 321E.1, 321E.2, 321E.28 and Iowa Code Supplement section 321E.8 as amended by 2002 Iowa Acts, Senate File 2192, section 36.