21—85.25(215) Air eliminator. All gasoline or oil metering devices shall be equipped with an effective air eliminator to prevent passage of air or vapor through the meter. The vent from such eliminator shall not be closed or obstructed.
This rule is intended to implement Iowa Code section 215.18.
[ARC 7129C, IAB 12/13/23, effective 1/17/24]
