875—155.5 (88B) Ten-day notices.
	 155.5(1) General. Permittees shall notify the division at least ten working days before an asbestos project begins. A project begins when site preparations for asbestos abatement, encapsulation, or removal begin; when asbestos abatement, encapsulation, or removal begins; or when any demolition begins, whichever is sooner. Facsimile transmissions of ten-day notices shall not be accepted.
	 155.5(2) Emergency. When there is an immediate danger to life, health or property, the permittee may file the notice within five days after beginning the project. An explanation of the emergency must be included.
	 155.5(3) Format. The notice shall be on an 8½″ by 11″ sheet of paper and shall contain the following information:
	  a.   	 The name, address, and telephone number of and contact person for the permittee performing the project.
	  b.   	 The name, address, and telephone number of the project.
	  c.   	 A description of the structure and work to be performed, including type and quantity of asbestos-containing material.
	  d.   	 The anticipated dates of the project’s start and end.
	  e.   	 Designation of the asbestos disposal site.
	  f.   	 The signature and printed name of the person who completed the form.
	  g.   	 The shift or work schedule on which the project will be performed.