761—162.2 (83GA,SF376) Definitions.
“Functionally obsolete” means the classification of a highway structure indicating one or more geometric features of the structure are below the standard required for current traffic. The classification is based on criteria established by the Federal Highway Administration in the “Recording and Coding Guide for the Structure Inventory and Appraisal of the Nation's Bridges.”
“Primary road system” means the same as defined in Iowa Code section 306.3.
“Structurally deficient” means the classification of a highway structure indicating one or more elements of the structure are in need of monitoring or repair. The classification is based on criteria established by the Federal Highway Administration in the “Recording and Coding Guide for the Structure Inventory and Appraisal of the Nation's Bridges.”
[ARC 8026B, IAB 8/12/09, effective 7/15/09]