567—101.408(455B) Temporary solid waste storage requirements. Unless otherwise specified within a permit, a solid waste transfer station shall comply with the following storage requirements.
    101.408(1) Areas permitted for storage. Solid waste shall be stored in the following manner.
    a.  Inside a solid waste transfer station building in a clearly marked designated area;
    b.  Inside a solid waste transfer station building in a surge pit;
    c.  Inside a secure solid waste transport vehicle, including intermodal container systems, protected from precipitation and vectors; or
    d.  Inside dumpsters, compactors, roll-off boxes, and other solid waste receptacles adequate to prevent the accidental discharge of its contents and the attraction or harborage of vectors.
    101.408(2) Storage time requirements. Solid waste shall be stored no longer than the following periods of time unless shorter storage times are required by the local government authority to prevent a nuisance or public health hazard.
    a.  Inside a solid waste transfer station building without a surge pit or similar operational structure for not more than four days, excluding Sundays and national holidays.
    b.  Inside a solid waste transfer station building in a surge pit for not more than seven days, including Sundays and national holidays.
    c.  Inside a solid waste transport vehicle designated to travel only via roadway for not more than four days, excluding Sundays and national holidays.
    d.  Inside a solid waste transport vehicle designated to travel via rail or navigable waterway, including intermodal container systems, for not more than seven days, including Sundays and national holidays.
    e.  Inside dumpsters, roll-off boxes, and other solid waste receptacles at registered solid waste transfer stations for not more than four days, excluding Sundays and national holidays.
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