567—102.207(455B) PCS storage areas. PCS shall be stored on an impervious surface, under a roof of tarp to minimize the infiltration of precipitation, or in an area with minimal potential for stormwater run-on.
[ARC 0483D, IAB 8/19/26, effective 9/23/26]
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