199—11.6 (478) Common and joint use.
	 11.6(1) Common use construction. Whenever an overhead electric line capable of operating at 69 kilovolts or more is built or rebuilt on public road rights-of-way located outside of cities, all parallel overhead electric supply circuits on the same road right-of-way shall be attached to the same or common line of structures unless the board authorizes, for good cause shown, the construction of separate pole lines.
	 11.6(2) Joint use construction. Rescinded IAB 5/14/03, effective 6/18/03.
	 11.6(3) Relocating of lines. When an electric supply line is to be constructed in a location occupied by an electric supply line or a communication line, the expense of relocating the existing line shall be borne by the utility proposing the new electric supply line. The electric utility proposing the new line shall not be required to pay any part of the used life of the existing line, but shall pay only the nonbetterment expense of relocating the existing line.