21—85.40(215A) Testing devices. All moisture-measuring devices will be tested against a measuring device that will be furnished by the department, and all moisture-measuring devices will be inspected to determine whether they are in proper operational condition and supplied with the proper accessories.
This rule is intended to implement Iowa Code section 215A.2.
[ARC 7129C, IAB 12/13/23, effective 1/17/24]